b75 to PUFF or LZMA conversion.

I want to Thank Jvvh first off for making all the conversion files and passing this on to us and also Ukronic for finding the proper way to convert to LZMA and PUFF among other things.

Both PUFF and LZMA can be done the exact same way but BOTH need to be done when reciever is already converted to b75.

NO NEED to load boot60 at all and actually can not be on boot60 to convert this way.

It's as simple as loading 2 bins using 2 different type Loaders.

Loaders needed GTRom Loader v27.02 [Pansat2700A - B75] or GTRom Loader v27A[pansat2700A] or Puff_BG_BOOT Loader Converter will work for loading LZMA or PUFF Boot BG bins.

FortecStarSTB or Blacklist Updater 1.4 or Blacklist Updater 1.3 Loaders for loading LZMA or PUFF 448k bins or whatever loader you used for b75 448k bins.

In How to I will use the loaders that I used for conversion but again any of the above loaders will work.
Quote: 	
How to Load.

(1). Open GTRom Loader v27.02 [Pansat2700A - B75] Loader.
Click Bin File , choose LZMA or PUFF Boot BG of choice.
Turn reciever ON.
Wait for reciever's front display panel to display ON or channel # , HIT Download.

Write should complete in 5 - 10 seconds then reciever will self reboot with either PUFF PUFF or PUFF. PUFF. depending on what conversion you have choosen then pause on F.

Turn reciever OFF from back switch.

(2). Open FortecStarSTB loader.
Click File , choose either LZMA or PUFF _258 bin.
Turn reciever ON wait for P hit Download.

After write is complete reciever will self reboot displaying PUFF PUFF, pause on F for 30-35 seconds then come ON then displaying channel #.
Thats it you are done.
	
Things to note that is very important.

If you choose LZMA Boot BG bin to convert, you MUST use LZMA bins.

If you choose PUFF Boot BG bin to convert, you MUST use PUFF bins.

You CAN NOT mix the two.

If converting to PUFF when turning reciever on front panel will display PUFF PUFF.

If converting to LZMA when turning reciever on front panel will display PUFF. PUFF.

Notice LZMA (PUFF.) has dot at end of F.

With PUFF or LZMA , loading conversion bins is actually easier.
With b75 you had to time it just right and most at first b.

With LZMA or PUFF you can actually let reciever cycle threw PUFF once and still be able to download bins.

Just need to do it before the second F appears.

You need to do this eventually and with 3 bins floating around things get confusing.
Some bins may get over looked from rushing them out for public release not getting the proper mods.
So to prevent this PLEASE convert to LZMA or PUFF.

If reciever is On Boot60 you will need to fully convert to b75 before converting to PUFF or LZMA this way or Use the 253(640k)_PUFF bin to convert to PUFF.

=======================================================