CW-650S Classic FTA Receiver The CaptiveWorks CW-650S Classic takes FTA receivers to a new level. With 32MB RAM, Component Video output, Optical Audio, and a Powerful Conexant Processor, this receiver leaves very little to be desired. 

Standard Features: 
- MPEG-2 Digital and Fully DVB-S Compliant
- SCPC/MCPC Receivable from C/KU band Satellite
- User Friendly OSD Menu with Full Function
- Installation by Easy Setup Guide
- 100 Satellites, 6000 Channels and 5000 transponders
- Brilliant On Screen Graphic
- Small Picture in Graphic and Zoom Function
- 8 Favorite Groups and Parent Lock Function
- EPG, including 7 days data fast download and timer
- Supports DiSEqC 1.0/1.2/1.3(USALS) and 22KHz Tone

Outstanding Value: 
- 256 Color Graphic User Interface
- Super Fast 800 Pages OSD Teletext Supported
- Multi Pictures Selection 4/9/10/12/13/16
- High Sensitivity QPSK Tuner and Demodulator
- Multi Timer Function and Favor
- Network Search and Easy Tuning
- Multi Languages: English/German/French/Italian/Spanish/Arabic/Turkish/Persian/Dutch
- Support 20 Audio PID (Language)
- Fast Channel Switching
- RS232 Port for Additional Information Service and Upgrading Software

Optional Features: 
- S-Video Output
- Zoom and Games
- Universal Remote Controller(TV/VCR/DVD/STB)
- CH3/CH4 RF Modulator with NTSC M 14-83

Technical Specification: 

Tuner 
Input Frequency 950MHz-2150MHz 
RF Input Signal Level -65 – 25dBm 
LNB Power 13/18V DC (+/-.5%), 0.5A max, overload protect 
DiSEqC 1.0/1.2/1.3 Tone Burst A/B 

RF Modulator: 
Output Level: CH3, CH4 
TV Standard NTSC 

Demodulator: 
Waveform QPSK 
Symbol Rate 1 to 45 M s/s 
FEC 1/2, 2/3, 3/4, 5/6, 7/8 
SCPC and MCPC Capable 

System and Memory: 
Main Processor Cx24142, Speed 160MHz 
Flash Memory 4MB 
SDRAM 32MB 

Back to top 

Audio Decoder: 
Audio Channel Mono, Dual Channel, Stereo, Joint Stereo 
Audio Mode mpeg-1/2 Audio layer I&II 
Sampling Freq 32/44.1/48KHz 

Video Decoder: 
Profile Rate MPEG-2MP@ML 
Input Rate Max. 15M bit/s 
Video System NTSC<->PAL converter 
Video Format 4:3, 16:9 (Letter Box) Pan&Scan 
Video Resolution 720x576 (PAL), 720X480 (NTSC) 

Power Supply: 
Input Voltage AC 100V-240V, 50/60MHz 
Power Consumption 25W Max 

Summary of Connectors: 
Audio Output 2xRCA(L/R) 
Video Output 1Xrca, S-VIDEO 
0/12V Output 1Xrca 
Serial Port RS232 9-Pin D-Sub, Male 
RF connector IEC Male to Female 

Physical Specification: 
Operating Temp 0 to 40 C 
Net Weight 1.8kgs 
Dimensions 280*235*56mm

File bellow

1- RS232 loader
2- factory software
3- Frist fix for nagra2 dn, bev, globecast and Telefonica (amazonas 61W) 
Attached Thumbnails