did post elsewhere that over the weekend I seem to have seen the DN prov start using 0x4a sized cmd07 packets again, but I'm still not that sure I saw real 0x6a sized cmd07 packets or if that was just an odd result of the old dg file. I was pretty sure when I started seeing 0x6a sized packets that it was something I was doing, and when the packets went away it was after doing key updates once I had the right combination of code that let AR work and stopped post-processing of ECMs so that that routine continued to work right.

Since I seem to be the only one testing it is hard to know if others see this stuff. Maybe if I read up in card coding section....
8/5/2008