Pansat 2500 - Pansat 2700 Converting Procedure 

First, here's a list of things that you need: 

- RS 232 female-female Straight Cable 
- A Pansat 2500 remote control 

Note : Before you start the conversion, please load the FACTORY BIN for Pansat 2500 into your receiver. 

Instructions/Procedure: 

- Please turn OFF your receiver and disconnect it from the satellite & the TV cable 
- Connect your receiver to your computer using RS 232 female-female Straight Cable 
- Now open the Blacklist STB Updater 1.4.0.0 
- Now, please select the "BIN" option on the Blacklist STB Updater 1.4.0.0 
- Now please select the correct "COM" port on the Blacklist STB Updater 1.4.0. 
- Now, please click the "Select Bin" button on the Blacklist STB Updater 1.4.0.0 
- Now, please look for the "j27_205_1.bin" file and click on it 
- Now, please turn ON your receiver and as soon as you see the first "dash light" on your receiver's front panel, click the "Write Bin" button on the Blacklist STB Updater 1.4.0.0 
- Now, please wait and let the bin download process complete 
- When it's done, your receiver will REBOOT automatically and soon you'll see B 7 5 flashes back and forth on your receiver's front panel 
- Now, please close the Blacklist STB Updater 1.4.0.0 window 
- Please turn OFF your receiver 
- Now re-open the Blacklist STB Updater 1.4.0.0 
- Now, please select the "BIN" option on the Blacklist STB Updater 1.4.0.0 
- Now please select the correct "COM" port on the Blacklist STB Updater 1.4.0. 
- Now, please click the "Select Bin" button on the Blacklist STB Updater 1.4.0.0 
- Now, please look for the "jvvh_208_1.bin" file and click on it 
- Now, please turn ON your receiver and as soon as you see the first "dash light" on your receiver's front panel, click the "Write Bin" button on the Blacklist STB Updater 1.4.0.0 
- Now, please wait and let the bin download process complete 
- When it's done, your receiver will REBOOT automatically and soon you'll see B 7 5 flashes back and forth on your receiver's front panel 
- That flashing B 7 5 will stop and freeze on number 5 for 30 seconds 
- After 30 seconds or so, your receiver will automatically boot (It'll turn ON automatically, after 30 seconds) 
- Now, please turn your receiver OFF and disconnect it from your computer 
- Finally, please connect the satellite and the TV cable to your receiver 
- That's It, you're done! Now, you’ve succussfully converted your FTA unit. 
- Finally, download the latest bin to your receiver (Read my Bin Loading Intructions file for help) 

Note: After you finish with the above steps, you have to re-scan your satellite(s). After you're done with that, you have to enter the latest keys (Dishnetwork or BellExpressVu). Here's what you need to do after you re-scan your satellite(s): 

- Go to MENU 
- Then, go to Parental Control / CAS Control Menu 
- Then, go to Second Pin and enter 0000 
- Then, go to Set Default Key 
- Then, go to Nagravision 2 to enter the latest Dishnetwork or BellExpressVu keys 

After you enter and store the latest keys, please EXIT the menu and start watching TV! 

Instructions provided by AV!