GENERAL FEATURES 
* Free To Air Channel Reception Only from Satellite and Terrestrial broadcasting
* IPPVR (Audio & Video recording to remote PC via LAN) 
* Dual Inputs (Satellite & Terrestrial) : 
-Fully Complies with ATSC HDTV (VSB) & DVB-S MPEG 2
-ATSC Tuner (LG NIM Type) & QPSK Tuner (LG NIM Type) 
-Decodes All ATSC HDTV Standard Video Formats 
Including 480i / 480p / 720p / 1080i 
-Selectable Output Video Format : 1080i / 720p / 480p / 480i 
-Standard Definition/High Definition contents 
(MPEG2 and support MPEG4 AVC/H.264) 
* 2 x USB 2.0, PVR Function Supported : Record & Play with an external HDD 
* High Definition Video Output : HDMI and Component (Y/Pb/Pr) 
* Audio Decoding : ISO/IEC13818-3(MPEG-2 audio/MUSICAM) Dolby AC-3 
* Full compliant of MPEG-S Digital & DVB broadcasting 
* 950-2150 MHz Input Frequency (IF Loop Throughout) 
* Satellite Scan – Multisat Scan support 
* Flexible reception of SCPC & MCPC from C/Ku-Band satellites 
* Variable input symbol rate 
* Video output resolution : 480p, 720p, 1080i 
* Various Aspect Ratio with4:3, Letter Box, Full Screen & 16:9 
* EPG (Electronic Program Guide) & Channels naming supported 
* Multi language OSD 
* Super fast channel changing speed 
* Over 6000 channels TV & Radio Program 
* Full Colors & User Friendly GUI for Easy Control 
* Timer function & PIG (Picture In Graphic) support 
* Zoom In-Out Function for Watching Screen 
* Moving Background for Protection of Plasma Display Panel & LCD TV in Radio CHs
* Powerful Various Downloding Methods 
-WebLoader downloading using ethernet port
-USB downloading using USB stick
-RS-232C cable downloading 
-Set to Set downloading (Main Program & Channel List Data File) 
* Powerful channel editing by 
- Sorting : Alphabetic, CAS, S-ID, TP order, All
- Move, Delete,Channel Rename, Channel Skip 
- 10 Favorite list & 200 programs per each list 
* Parental Lock Function using Master PIN Code 
* Satellite & TP / Network Scan 
* DiSEqC 1.0, 1.1, 1.2 & USALS / 22KHz Switching Control Supported 
* Comparable of setting the frequency for SMATV system 
* Super universal remote 
* UHF ready
* Fast and Smart Scan
* High LNB power generation 

TECHNICAL SPECIFICATION 
* Satellite 
- 1 Input Connector : F-type,IEC 169-24 
- IF Input Frequency : 950MHz to 2150MHz 
- IF Loop Throughout : 950MHz to 2150MHz 
- Input Level : -65 dBm~-25 dBm 
- DiSEQqC Control : 1.0, 1.1,1.2 & USALS Compatible 
- Band Switch : 22KHz Tone(22 +/- 4KHz. Amplitude : 0.6 +/- 0.2V) 
- Symbol Rate : DVB-S QPSK : 1-45Msps
- Viterbi Decoding Rate : 1/2, 2/3, 3/4, 5/6 and 7/8 
- Bandwidth : 36MHz 
- LNB Power : 13 /18VDC / 1,000mA Max 
* Terrestrial
- ATSC A/53 compliant, 8/16VSB and MMDS, 2/4/8VSB receiver, ITU-U, J.83 Annex B/C, SCTE, DVS-031 compliant, 64/256QAM receiver 
* Power
- Input Voltage : AC 100~250V, 50/60Hz 
- Power Consumption : Max. 45 Watts 
- Power Supply Type : SMPS 

MPEG TRANSPORT STREAM A/V DECODING
* Demultiplex : According to ISO/IEC 13818-1(MPEG-2 system) 
* Input syream : Max. 90Mbit/s 
* Aspect Ratio : 4:3, 16:9 
* Video Resolution : 480p or 720p, 1080i 
* Audio Decoding : ISO/IEC13818-3(MPEG2 Audio/MUSICAM),Dolby AC-3 
* Audio Mode : SingleChannel/Dual Channel, Stereo, Joint Stereo 
* Video Output : HDMI,Component, RCA, S-Video

MICROPROCESSOR & MEMORIES 
* Main Processor : STI 7101 
* CPU Clock : 266Mhz 
* Flash Memory : 4 Mbyte + 1Gbyte (Nand flash memory) default 
(16Gbyte nand flash memory : Optional) 
* DDR SDRAM : 192 Mbyte 
* EEPROM : 32 Kbit(Optional) 

DATA PORT 
* Serial : 9 Pin D-Sub Type Connector
RS232 Asynchronous , 
Data Rate Max :115.2Kbps
* Ethernet : 10BaseT/100BaseTX 
* USB : 2.0 High speed

A/V OUTPUT
* Digital output : HDMI
* Video : Y/Pb/Pr, CVBS output (RCA)
* Audio : Stereo L/R output (RCA)
* S-VHS : S-Video 
* Digital Audio : 1 optical output, S/PDIF

FRONT PANEL 
* Smart Card : 1 Slot 
* 7 keys : Menu, OK, Power, Channel Up/Down, Volume Up/Down 
* Integrated USB 2.0 (Front side) , support to USB memory stick and USB HDD
* Green VFD display (moving 12 characters in 1 line) 

REAR PANEL 
* ATSC Signal INPUT 
* Loopthrough output 
* S-VHS : S-Video 
* IF Input & Out
* 3RCA : Video, Audio L, Audio R 
* Component output : Y/Pb/Pr
* UHF Optional Signal In
* Ethernet port
* Integrated USB 2.0 (Rear side), support to USB memory stick and USB HDD 
* HDMI Connector : Type A 
* S/PDIF for Digital Audio AC-3 Bitstream Output 
* RS232 Serial Port : 9 Pin Connector, D-Sub Type, Twisted Cable
* Built-in Internal Cooling Fan 
* Power On/Off switch 

REMOTE COTROL 
* Type : Super Universal Remote Control
* Battery : 2x1.5V AAA Type 

DIMENSIONS AND WEIGHT 
* Size : 13.4 (W) x 9.65 (D) x 2.36 (H) [inch], (340 (W) x 245 (D) x 60 (H) [mm]) 
* Weight (Net) : 5.95 lbs, (2.7 kg) 		
￹FPRIVATE "TYPE=PICT;ALT=Nfusion Specs"