Tronics Bin Modifier version 1.1 

Hello everyone,

I have received numerous requests for a new version of my bin converter/modifier program. I had stated before that I would not be releasing a new version because of certain negative behaviors that resulted from the first release. Many people had very nice things to say and basically said not to let a few people spoil it for everyone. Well I think I have come up with a solution that will work for all. I have a new and greatly improved version of my program that I will now release. This version is quite different from the 0.7 version. The new version is ver1.1 and it has the following features:

1.) It now has a GUI. In fact it now MUST be run from the GUI, no more command line.
 1.) Esta ahora tiene auna GUI, La verdad, esta debe de ser usada (corrida) desde la GUI, no mas comandos.

2). There are no longer any output files. This program will NOT generate bins that you can then pass around and load via any loader you want. All modifications are done in program.
2.Ya no habran mas bines plagiados(mi forma de decirlo)>este programa no generara bines que tu puedas pasar como tuyos y load via cualquier loader
que  quieras usar.Todas las modificaciones seran hechas dentro del programa

3) I have included a loader into this version. Due to item 2 it is now mandatory to use this program to both modify and load the bin into your receiver.
 3) Con esta version yo he incluido un Loader ",Debido  a mi Bin modificador ahora es obligacion  usar este programa para mods y load el en tu reciver
  
4) This version supports more receivers. The old version only did PUFF conversions. This version now works for the following receivers:
PUFF converted receiver.
 PUFF convertidos reciveres

4)Esta version suporta mas reciveres. The version anterior solamente se podian ha*cer conversiones PUFF.Esta trabaja para los siguientes reciveres:
B75 using LH5 compression converted receivers
B75  que estan usando la compresion LH5 en convertidos reciveres

2700 clone receivers using stock B75 boot without any compression
2700 clones usando B75 boot sin ninguna compresion( solo removiendoles el clone kill)

Converted Ariza receivers
Arizas convertidos a pansats, (Pariza) La mods tool trabaja bien para todos estos bines

The first two have been well tested. The last two have been tested by others and have been reported to work but I would like to hear some feedback regarding these new additions.
En los dos primeros han sido probados bastante (buenos resultados)En los 2 ultimos han sido tested y los reportes dicen  que trabajan bien.
pero me gustaria que me reportaran y tener opiniones respecto a estan nuevas adiciones.

5) The program can now also load the b75 with LH5 compression or the PUFF boot to the receiver.
5)El Programa (Nuevo programa loader) puede tambien load el B75 bin con la compresion LH5 o el bin PUFF  al reciver.

6) For PUFF converted boxes only, you may now use this program to change the text displayed by the receiver on boot. I made this available only to PUFF boots so as to minimize confusion regarding which boot a receiver is running. If your receiver displays non-standard text on boot then it is converted to PUFF.
6)  Para las cajas convertidas a PUFF, ahora tu puedes usar este programa para cambiar el texto  que se ve en el reciver cuanto este se reboot.Esto solo es posible en la PUFF boot, para minimizar la confusion debido a cual boot el reciver esta usando.Si tu reciver muestra un no standard texto(diferente) cuando se reboot,entonces este es un convertido a PUFF(usara puff bines)..

7) The program now allows you to change the background image, for all receivers. For PUFF converted receivers the image may be placed in either the boot section or the main program section. If put in the main program section, however the image size is limited to just under 10K bytes (9882 bytes). If placed in the boot section the image size may be significantly larger. (keep in mind though that with MPEG1 bigger is NOT better. You will often get a better looking image with a smaller input file.)
 7) Esto esta explicado en el otro texto, es sobre la background imagen,( indicando que mas grande la imagen no es mejor en MPEG1, que se obtiene mejor imagen con un file pequeno(la imagen).

8) This program can now remotely reset your receiver. As long as your receiver is powered up and fully boot and has the serial cable attached you can use this program to flash the receiver without having to manually power cycle to box. This should allow for greater flexibility in programming and hopefully eliminate the race condition that is inherent in the current programming procedure (i.e. waiting for first P or b then clicking download)
8) Ahora este programa  puede a control remoto reset tu reciver(Load)iempre que el reciver este encendido y completamente boot up y tenga el  serial cable      
  conectado, tu podras usar este loader para flash tu reciver sin tener que  apagar y encender la caja(como normalmente lo ha*cemos, "nota mia")

9) The error messages are much more informative. There will not be any messages like 'error 1' or the like. If you receive an error message it will tell you exactly what the error was, at which stage of the process the error occurred and what to do to remedy it. I have seen so so many people asking the same types of questions in the forums and I keep giving the same answers over and over again. Now I have incorporated those common answers into the error messages so hopefully people will be able to more easily troubleshoot problems as they arise.
9
Los mensajes de errores  dan mas informacion. No habra ningun mensaje como "error 1" o parecidos. Si tu recives un mensaje de error,este dira cual
es el error, en que paso del proceso el error ocurrio y que ha*cer para remediarlo,He visto tantas personas haciendo el mismo tipo de preguntas
en los foros y Yo todavia sigo dando las mismas respuestas una y otra vez.Ahora yo he incorporado esas re4spuestas comunes en los mensajes 
de errores  con la esperanza que las personas  sean capaces de mas facilmente solventar los problemas  cuando estos aparezcan.

10) The loader will automatically modify the protocol used dependent on the type of file/receiver selected by the user. You don't have to specify which command set to use, the loader is smart enough to determine that for you.

10) El loader  automaticamente modificara el protoclo usado,dependiendo en el tipo de file/reciver seleccionado por el usuario.Tu no tendras que especificar  cual comando usar,el Loader es suficiente inteligente ,el lo hara por ti

11) The program comes complete with a nice integrated help file with some FAQs, at least questions that I expect may be frequently asked.
 That is all I can think of,hopefully I have bot omitted anything.
11) El programa viene con un muy bien integrado file de ayuda con algunas FAQs( factores, respuestas,y Preguntas) Esas son todas de las que yo  puedo
pensar por ahora. Espero que no haya omitido ninguna

la parte de abajo, se refiere a que si PC no tiene  el NET framework instalado en tu PC, tienes que instalarlo
bajandolo de la liga que el tiene en el paquete que el posteo para que el loader y la tool trabajen.

This part is in bold and underlined for a reason!!! If you get an error message when you try to launch the application that says 'The application failed to initialize properly (0xc0000153)' this means that you need to install the .NET framework. I wrote this program in visual C++ .NET and therefore it depends on the .NET framework to function. I was going to include the .NET framework with the release but it is 3 times the size of my program and many computers will already have the .NET framework installed, so to try to conserve bandwidth I have included an html file named 'GetDotNetFramework.html'. If you get this error just double click this file and it will download the required .NET framework setup file for you. Then run that program called dotnetfx3setup.exe and it will install the .NET framework on your system. After that has been done the program will run as it should.
Esta parte esta  en letras grandes y negras ,ademas  subrayadas por una razon!! Si  tu obtienes un  "error"mensaje cuando uses esta aplicacion que dice:The application failed to initialize properly( La aplicacion fallo )(0xc0000153)  Esto significa que tienes que instalar el .NET framework,Yo escribi este programa en visual C++.NET  y por esa razon  depende de .Net framework para que funcione. Yo iva a incluir con el file que saque ,pero este es 3 veces mas grande que mi programa y muchas computadoras ya tienen el .Net framework instalado.por eso trate de conservar bandwidth (banda ancha"rate de data transfer").Yo he incluido un file nombrado"GetDoNetFramework.html". Si tu obtienes este error,solamente doble click este file(en el programa que bajes, no esta ,"no trabajara" nota mia) y este sera downloaded la requerido .NET framework sertup file para tu uso.Entonces "run "el programa llamado dotnetfx3setup.exe y este instalara el .NET framework en tu computadora.Despues que hagas eso el programa funcionara como debe de ser.

For background images, you need to convert your desired image to MPEG1 format. The program TMPGENc is well suited to this task and is free. Unfortunately, TMPGENc does not allow unauthorized distribution of this software so I couldn't bundle it with my release. That being said there is a link to their site located in the Help page within my program. If you want to use TMPGENc just click the help tab from within the program and click the TMPGENc link. A new browser will open and take you to the download page.
Para las background imagenes,tu necersitas convertir tu imagen escojida a MPEG1 formato.El programa TMPGENc es el mas indicado para esto y es gratis.    Desafortunadamente,TMPGENc,no permite  unactorizada destribucion de este softare(programa),por esta razon  no pude incluirlo en mi paquete.Por esta razon  que digo,ahi hay una liga,esta esta localizada en la pagina de Help (ayuda) dentro de mi programa(para mods bins) Si tu quieres usar TMPGENc solo click en la ayuda tab en el programa y click en la  TMPGENc liga  un nuevo browser se abrira y este te llevara a la pagina de download.

I have included various cryptographic safeguards to avoid people tampering with my program and its constituent files. ANY modification to any of the files will result in the program ceasing to function. 
YO he incluido varias criptograficas protecciones para evitar que la gente no cambie nada en mi programa y en los files que lo componen.Cualquier modificacion a cualquiera de los files resukltara que el programa deje de funcionar.

Although this program has been tested by a number of individuals prior to release I must state that this is a USE AT YOUR OWN RISK PROGRAM
I don't expect any problems but I must make it clear that I take no responsibility if anything bad happens to your receiver as a result of using my program. 
Debido a que este programa a sido probado por varios individuos  antes de postearlo debo decir que este es un Usa a tu propio riesgo programa. Yo no espero que tengan ningun problema,pero  quiero dejar bien claro que yo no asumo ninguna responsabilidad si algo le pasa a tu reciver como un resultado de usar este  programa.

I hope everyone values and enjoys this new contribution and if there are any issues please politely let me know and I will try to remedy them ASAP.
Espero que todo mundo valore y disfrute esta nueva contribucion y si encuentras algun problema por favor dimelo muy cortesmente que yo tratare de remediarlo ASAP tan pronto como me sea posible..

Best Regards,

Tronics
si alguien puede hacer esto mas simple, bienvenido ,de eso se trata, mas simple,mejor. hermosillo sonora