"pregunta. en el menu de mi reciver  no esta el  icon de la internet, pero atras de la caja
tiene  el port de la eternet,ayuda,necesito poner a funcionar esta caja, 
on my receiver menu mine doesn't have the internet icons,but on the back of my box it has the ethernet port help need to get this box up and running	
Respuesta

Step 1: Connect your Nfusion to your PC using the null modem cable
            conecte tu nfusion a tu PC usando el null modem cable.

Step 2: Set loader to load boot file
            Set el loader a load  boot file.

Step 3: Load the 130 boot file, at completion of load the display should read "Good" not "NEnu"
             load el 130 boot file, cuando la download se complete se leera "Good" no "NEnu

Step 4: Change loader option to now load a bin file
              Cambia loader opcion ahora a bin file.

Step 5: Load the 144 bin
            Load el bin 145.2    ( es mas nuevo) 

Step 6: Disconnect your Nfusion from your PC 
            Desconecta tu nfusion de la PC.

Step 7: Connect to TV check the S/W version which should read boot 130 and bin 144
           Conecta este a la tv, el s/w version que debera leerse seria  boot 130 y bin 144( si le pones el 144)

(To Check S/W go Menu-->System Setting-->S/W Version)
 Para revisar la version ve a  Menu-->System setting-->S/W Version

Step 8: Finish antenna set-up
           Setup tus antenas etc.
Step 9: Connect to router and finish network set-up
           conectalo al router(si tienes) y has el network se-tup

Step 10: Have cold beer and watch TV